
**Proper Steps to Taking an X-Ray**


------------------------------------------

1. BEFORE YOU LOG IN insert the sensor
2. Log into the computer but DO NOT OPEN ANY SOFTWARE YET
3. Wait a few seconds for this bubble in the bottom right corner to pop up:




1. A few seconds later another bubble will appear…

Schick:



Kodak:



1. Launch axiUm/MiPACS

If you are still experiencing issues after following the steps above, please call IT at 215-898-8957! Thank you!